MX or Fruehauf insulation test  
Take the Load cell cable into the mother board.  
There are 5 wires per load cell.   
These are: Positive and Negative Power  
Positive and Negative Display Reading  
Yellow: Earth.  
Set the Fluke Tester to 50V  
Red cable into the V Insulation on the tester  
Black cable into the COM on the front of the tester  
Attach black to a bare piece of chassis metal   
Attach red on a crocodile to a bundle of 4 of the 5 wires (NOT THE YELLOW)