MX or Fruehauf insulation test
Take the Load cell cable into the mother board.
There are 5 wires per load cell.
These are: Positive and Negative Power
Positive and Negative Display Reading
Yellow: Earth.
Set the Fluke Tester to 50V
Red cable into the V Insulation on the tester
Black cable into the COM on the front of the tester
Attach black to a bare piece of chassis metal
Attach red on a crocodile to a bundle of 4 of the 5 wires (NOT THE YELLOW)